

![](data:None;base64,)

Smartphone app for the control of a radar exposimeter

Type of Thesis

Presented by: Remo Steiner, Matthias Stähli, André Eggli, Markus Reichmuth

Supervised by: Marco Zahner

Prof. Dr. Juerg Leuthold

December 2016

Table of Contents

[Table of Contents 3](#_Toc468976637)

[1 Introduction 4](#_Toc468976638)

[2 Theory 5](#_Toc468976639)

[2.1 Data transmission 5](#_Toc468976640)

[2.2 Data processing 5](#_Toc468976641)

[2.3 Data flow 5](#_Toc468976642)

[2.4 Data Plot 5](#_Toc468976643)

[2.4.1 Heading 3 5](#_Toc468976644)

[2.4.1.1 Heading 4 5](#_Toc468976645)

[3 Results 6](#_Toc468976646)

[3.1 Handbook 6](#_Toc468976647)

[3.1.1 General 6](#_Toc468976648)

[3.1.1.1 Hotspot configuration 6](#_Toc468976649)

[3.1.1.2 Connection lost 6](#_Toc468976650)

[3.1.2 Home Screen 6](#_Toc468976651)

[3.1.3 Overview 7](#_Toc468976652)

[3.1.4 Detail view 7](#_Toc468976653)

[3.1.5 Timeline 7](#_Toc468976654)

[4 Summary 9](#_Toc468976655)

[5 References 10](#_Toc468976656)

[Appendix A: List of Symbols 11](#_Toc468976657)

The first chapter has three purposes

* What are the challenges? Why is this thesis needed?
* State-of-the art: Discuss as of what was the state-of-the art at the beginning of the thesis. Has there been progress by other groups? Give key citations.
* What are the results offered by this thesis? To what extent have the challenges been tackled by this thesis. Summarize the key results.

# Introduction

Radar signals consists of short and very powerful pulses. In some cases, the peak power of a transmitted burst can reach very high values compared to the ones from telecommunication base stations. Meanwhile, the use of very short duty cycles and the rotation of a radar Antenna lead to comparatively low average power values. Due to the huge differences between the average and the peak field near radar stations, a commercially available exposure meter is not suitable to correctly differentiate these two field values. Hence, there is a need for a device, which is capable of measuring both fields precisely. The Institute of Electromagnetic Fields (IEF) at the ETH Zurich developed therefore a display-less, portable tool, called “Exposimeter”. In order to control this device and to plot the measured data, there is a demand for a smartphone app. In an early stage, a first application provided the plotting of single frequencies without the ability to control the exposimeter. The lack of the capacity to regulate the device and the fact that a newer version of the exposimeter did no longer provide the connection over Bluetooth but over Wi-Fi lead to a development of a new app.

# Requirements

The requirements of the app are:

* Connect to the device over Wi-Fi
* Processing and plotting data
* Controlling the Exposimeter
* Android based

The app consists of three different plotting types:

* Overview: A measurement over a big range of frequencies, to show the outstanding values of either peak or RMS fields.
* Detail view: One to six frequencies can be chosen separately for further investigation. The corresponding values, both peak and RMS, are plotted in a new window.
* Timeline: To display one of these selected frequencies in real time.

The Exposimeter has four different attenuation levels which can be set by the application:

* Normal mode
* -42dB
* -21 dB
* LNA

Further information provided by the app:

* Battery level of the exposimeter device
* Device number

# Functional blocks

The second chapter typically introduces the theory subsequently needed. It will allow a reader in the field to read the next chapters without looking up books. Key results and derivations are given. The theory may be derived from literature – but proper citing is expected. The material however has to be made up in a consistent way and a common nomenclature has to be used throughout the thesis.

The chapter should give both an overview on the theory and its context but also an in-depth idea of the formulas used in the next chapters.

## Matlab

## Data transmission

## Data processing

## Data flow

## Data Plot

### Heading 3

Text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text.

|  |  |  |
| --- | --- | --- |
|  |  | (2.5) |

Text text text text text text text text text text text text text text text.

#### Heading 4

Text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text, see (2.5).

# Results


This chapter comes with results. Published papers may be copied without any additional modifications into the text. Equations and Figure captions however should be adapted to the style of the thesis. A paper that is copied into the thesis must be cited with its original reference and all coauthors.

## User manual

### General

#### Hotspot configuration

The data is passed between the exposimeter device and the smartphone over Wi-Fi. The smartphone plays the role of a master, the exposimeter the one of a slave. Therefore, the smartphone must offer a hotspot for the connecting device. The configuration must be adjusted before opening the app. To configure the hotspot, follow these steps: Settings -> Wireless & networks -> Tethering & portable hotspot -> set up Wi-Fi hotspot. Set up the network name and password as showed in Fig 3.1. Then enable Portable Wi-Fi hotspot. If the hotspot isn’t enabled, the app will store the current network state and enable the Wi-Fi hotspot on starting and reset the network state on closing. Note that this is only working, if the airplane mode is not enabled.





#### Connection lost

If the connection between the smartphone and the exposimeter device is lost, a red bar will show on the top. To fix this error, close the app, check the connection and restart the app.

### Home Screen

On first starting the app, the hotspot configuration will be enabled and a trigger packet will be sent automatically to the exposimeter device, which then returns all calibration tables for each of the four different attenuation modes. A progress bar is indicating the progress of the transmission. After receiving all calibration spreadsheets, one can choose between the four attenuation modes. On the top left, the battery level of the exposimeter device and its device ID is displayed, see Fig 3.2.



### Overview

On clicking on one of the attenuation modes, a new window will open and show a plot of all frequencies, ranging from 500 to 10000. On the right hand side, there are six buttons for further interaction:

* After selecting an interesting frequency by pressing on the corresponding frequency-bar, this selected frequency is added in a pool for further investigation. A maximum of six different frequencies can be chosen and added each separately to this pool. The bars shown in green are already selected, while the bar shown in red can be added to the pool by pressing the plus button.
* For the selected green bars, a new window opens in the Detail view.
* Each selected frequency can be deleted from the pool one by one.
* To refresh the whole overview plot, one can use the refreshing button.
* The overview plot is either showing the peak or the RMS measurement. The yellow button is for switching between these two states. The current configuration can be seen in the top left corner.
* On pressing on the configuration button, one can see and change the current attenuation mode.

### Detail view

After selecting some frequencies and pressing the green arrow button, a new window opens in the Detail view. The Peak and RMS value of all chosen frequencies are shown. On pressing on one single frequency, the timeline window will open for this selected frequency. On the right side, there are two buttons for interaction:

* The Peak and RMS values are updated from time to time. To stop this refreshing, one can press the yellow stop button. Another press on the same button will restart the updating.







* On pressing on the configuration button, one can see and change the current attenuation mode.

### Timeline

The timeline view plots one single frequency over time. The frequency can be selected in the Detail view. A yellow bar is swiping through the chart, indicating the current measured value. To inspect the RMS and Peak value at a specific time, one can select a bar, which will then appear in green. On the right side, there are the same two buttons as in the Detail view for interaction:

* The Peak and RMS values are updated from time to time. To stop this refreshing, one can press the yellow stop button. Another press on the same button will restart the updating.
* On pressing on the configuration button, one can see and change the current attenuation mode.



Text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text, see Fig. 3.1.



Fig. 3.1: Caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption.

# Summary

Summarize the thesis. Give results and give numbers as to what has been achieved.

Vision – tell the bigger vision of what might come next and how the world is going to change if the results are realized.

The outcome of the project is a well-functioning, simple to handle and purposeful app, as it was expected. The app is capable to connect easily with the exposimeter device, getting data, process and parse these data and plot it in a clear way. The key features are three different plotting types, which provides suitable information about the peak and average field.

For further improvement:

* Battery
* More stable, better working code

# References

[1] G. P. Agrawal, *Fiber-optic communication systems*, 2nd ed. New York, N.Y.: Wiley, 1997.

[2] W. H. Press, *Numerical recipes in C the art of scientific computing*, Second ed. Cambridge etc.: Cambridge University Press, 1999.

[3] S. V. Kartalopoulos, *DWDM networks, devices, and technology*. Piscataway, NJ: IEEE Press, 2003.

[4] A. Leon-Garcia and I. Widjaja, *Communication networks fundamental concepts and key architectures*. Boston, Mass.: McGraw-Hill, 2000.

[5] F. Frhr. v. Loeffelholz, "Pionier der Informationstheorie Claude Elwood Shannon," *c't - Magazin für Computertechnik,* vol. 6/2001, 2001.

[6] P. J. Winzer, "Modulation and Multiplexing in Optical Communications," in *Conference on Lasers and Electro-Optics/International Quantum Electronics Conference*, Baltimore, Maryland, 2009, p. CTuL3.

[7] W. Freude, R. Schmogrow, D. Hillerkuss, J. Meyer, M. Dreschmann, B. Nebendahl*, et al.*, "Reconfigurable optical transmitters and receivers," 2012, pp. 82840A-82840A-8.

[8] *Twisted-Pair-Kabel*. Available: <http://de.wikipedia.org/wiki/Twisted-Pair-Kabel>

[9] *Kabel - nicht nur für den Computerbau wichtig*. Available: <http://www.hardware-bastelkiste.de/index.html?cable.html#TP%E2%80%9C>

[10] A. Leon-Garcia and I. Widjaja, "Twisted Pair," in *Communication networks fundamental concepts and key architectures*, ed Boston, Mass.: McGraw-Hill, 2000, p. 148.

[11] T. Kremp and W. Freude, "DWDM transmission optimization in nonlinear optical fibres with a fast split-step wavelet collocation method," in *7th International Conference on Optoelectronics, Fiber Optics & Photonics (Photonics)*, Kochi, India, 2004.

[12] R.-J. Essiambre, G. J. Foschini, P. J. Winzer, and G. Kramer, "Capacity limits of fiber-optic communication systems," in *Proc. Opt. Fiber Commun. Conf.*, San Diego, CA, 2009.

[13] *Video broadcasting technology*. Available: <http://www.epanorama.net/links/videobroadcasting.html>

[14] *High-definition television*. Available: <http://en.wikipedia.org/wiki/High-definition_television>

[15] P. Qu and C. Polley. (2005). *The New Standard-Bearer: China is now trying to set the rules for many developing technologies*. Available: <http://spectrum.ieee.org/computing/hardware/the-new-standardbearer>

[16] D. Santa-Cruz and T. Ebrahimi, "A study of JPEG 2000 still image coding versus other standards," *Proc. of the X European Signal Processing Conference,* vol. 2, pp. 673-676, 2000.

1. List of Symbols

Text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text.

Text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text.