

![](data:None;base64,)

Smartphone app for the control of a radar exposimeter

Type of Thesis

Presented by: FirstName LastName

Supervised by: FirstName LastName

FirstName LastName

Prof. Dr. FirstName LastName

Month YYYY

DISS. ETH NO. XXXXX

Title Title Title Title Title Title Title Title Title Title Title Title Title Title Title Title Title Title Title Title Title Title Title

A thesis submitted to attain the degree of

Doctor of Sciences/Master of Science/Bachelor of Science of ETH Zurich

(Dr. sc. ETH Zurich/MSc ETH Zurich/BSc ETH Zurich)

presented by

FirstName LastName

MSc EEIT/BSc EEIT, name of university

born on dd.mm.yyyy

citizen of Heimatort(Swiss citizens)/Nationality(foreign citizens)

accepted on the recommendation of

Prof. Dr. FirstName LastName, examiner

Prof. Dr. FirstName LastName, co-examiner

Prof. Dr. FirstName LastName, co-examiner

20XX

Table of Contents

[Table of Contents 3](#_Toc468976637)

[1 Introduction 4](#_Toc468976638)

[2 Theory 5](#_Toc468976639)

[2.1 Data transmission 5](#_Toc468976640)

[2.2 Data processing 5](#_Toc468976641)

[2.3 Data flow 5](#_Toc468976642)

[2.4 Data Plot 5](#_Toc468976643)

[2.4.1 Heading 3 5](#_Toc468976644)

[2.4.1.1 Heading 4 5](#_Toc468976645)

[3 Results 6](#_Toc468976646)

[3.1 Handbook 6](#_Toc468976647)

[3.1.1 General 6](#_Toc468976648)

[3.1.1.1 Hotspot configuration 6](#_Toc468976649)

[3.1.1.2 Connection lost 6](#_Toc468976650)

[3.1.2 Home Screen 6](#_Toc468976651)

[3.1.3 Overview 7](#_Toc468976652)

[3.1.4 Detail view 7](#_Toc468976653)

[3.1.5 Timeline 7](#_Toc468976654)

[4 Summary 9](#_Toc468976655)

[5 References 10](#_Toc468976656)

[Appendix A: List of Symbols 11](#_Toc468976657)

# Introduction

The first chapter has three purposes

* What are the challenges? Why is this thesis needed?
* State-of-the art: Discuss as of what was the state-of-the art at the beginning of the thesis. Has there been progress by other groups? Give key citations.
* What are the results offered by this thesis? To what extent have the challenges been tackled by this thesis. Summarize the key results.

The state-of-art at the beginning of the work was, that

The aim of this group work is to develop an android based app, which displays data, provided by a radar signal measure instrument. The radar exposimeter is a self-assembled, display-less, portable device. Its focus is especially on peak values of radar signals, due to the huge differences between the average and the peak field near radar stations. The measured data are digitalized by a microcontroller which is connected to a Wi-Fi module. Data is there passed to a smartphone, where it is received, processed and plotted in the app.

The app consists of three different plot settings:

* Overview: A measurement over a big range of frequencies is made, to show the outstanding values of either peak or RMS fields.
* Detail view: One to four frequencies can be chosen separately for further investigation. The corresponding values, both peak and RMS, are plotted in a new window.
* Timeline: To display one of these selected frequencies over ten seconds, the user can switch to the timeline view.

As a presetting, one out of four different measurement levels can be chosen:

* Normal mode
* -42dB
* -21 dB
* LNA

Further showed information are:

* Battery level of the exposimeter device
* Device number

The state-of-art at the beginning of the work was, that there was an already existing app, corresponding to an older version of the exposimeter instrument. The connection was based on Bluetooth technology. Due to the fact, that the measurement device was rebuilt and equipped with a Wi-Fi module, there was a need of an updated app. After careful consideration, it was decided to not improve the existing app, but to develop a new one.

# Requirements

# Functional blocks

The second chapter typically introduces the theory subsequently needed. It will allow a reader in the field to read the next chapters without looking up books. Key results and derivations are given. The theory may be derived from literature – but proper citing is expected. The material however has to be made up in a consistent way and a common nomenclature has to be used throughout the thesis.

The chapter should give both an overview on the theory and its context but also an in-depth idea of the formulas used in the next chapters.

## Matlab

## Data transmission

## Data processing

## Data flow

## Data Plot

### Heading 3

Text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text.

|  |  |  |
| --- | --- | --- |
|  |  | (2.5) |

Text text text text text text text text text text text text text text text.

#### Heading 4

Text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text, see (2.5).

# Results


This chapter comes with results. Published papers may be copied without any additional modifications into the text. Equations and Figure captions however should be adapted to the style of the thesis. A paper that is copied into the thesis must be cited with its original reference and all coauthors.

## User manual

### General

#### Hotspot configuration

The data is passed between the exposimeter device and the smartphone over Wi-Fi. The smartphone plays the role of a master, the exposimeter the one of a slave. Therefore, the smartphone must offer a hotspot for the connecting device. The configuration must be adjusted before opening the app. To configure the hotspot, follow these steps: Settings -> Wireless & networks -> Tethering & portable hotspot -> set up Wi-Fi hotspot. Set up the network name and password as showed in Fig 3.1. Then enable Portable Wi-Fi hotspot. If the hotspot isn’t enabled, the app will store the current network state and enable the Wi-Fi hotspot on starting and reset the network state on closing. Note that this is only working, if the airplane mode is not enabled.





#### Connection lost

If the connection between the smartphone and the exposimeter device is lost, a red bar will show on the top. To fix this error, close the app, check the connection and restart the app.

### Home Screen

On first starting the app, the hotspot configuration will be enabled and a trigger packet will be sent automatically to the exposimeter device, which then returns all calibration tables for each of the four different attenuation modes. A progress bar is indicating the progress of the transmission. After receiving all calibration spreadsheets, one can choose between the four attenuation modes. On the top left, the battery level of the exposimeter device and its device ID is displayed, see Fig 3.2.



### Overview

On clicking on one of the attenuation modes, a new window will open and show a plot of all frequencies, ranging from 500 to 10000. On the right hand side, there are six buttons for further interaction:

* After selecting an interesting frequency by pressing on the corresponding frequency-bar, this selected frequency is added in a pool for further investigation. A maximum of six different frequencies can be chosen and added each separately to this pool. The bars shown in green are already selected, while the bar shown in red can be added to the pool by pressing the plus button.
* For the selected green bars, a new window opens in the Detail view.
* Each selected frequency can be deleted from the pool one by one.
* To refresh the whole overview plot, one can use the refreshing button.
* The overview plot is either showing the peak or the RMS measurement. The yellow button is for switching between these two states. The current configuration can be seen in the top left corner.
* On pressing on the configuration button, one can see and change the current attenuation mode.

### Detail view

After selecting some frequencies and pressing the green arrow button, a new window opens in the Detail view. The Peak and RMS value of all chosen frequencies are shown. On pressing on one single frequency, the timeline window will open for this selected frequency. On the right side, there are two buttons for interaction:

* The Peak and RMS values are updated from time to time. To stop this refreshing, one can press the yellow stop button. Another press on the same button will restart the updating.







* On pressing on the configuration button, one can see and change the current attenuation mode.

### Timeline

The timeline view plots one single frequency over time. The frequency can be selected in the Detail view. A yellow bar is swiping through the chart, indicating the current measured value. To inspect the RMS and Peak value at a specific time, one can select a bar, which will then appear in green. On the right side, there are the same two buttons as in the Detail view for interaction:

* The Peak and RMS values are updated from time to time. To stop this refreshing, one can press the yellow stop button. Another press on the same button will restart the updating.
* On pressing on the configuration button, one can see and change the current attenuation mode.



Text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text, see Fig. 3.1.



Fig. 3.1: Caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption caption.

# Summary

Summarize the thesis. Give results and give numbers as to what has been achieved.

Vision – tell the bigger vision of what might come next and how the world is going to change if the results are realized.

The outcome of the project is a well-functioning, simple to handle and purposeful app, as it was expected. The app is capable to connect easily with the exposimeter device, getting data, process and parse these data and plot it in a clear way. The key features are three different plotting types, which provides suitable information about the peak and average field.

For further improvement:

* Battery
* More stable, better working code

# References

[1] G. P. Agrawal, *Fiber-optic communication systems*, 2nd ed. New York, N.Y.: Wiley, 1997.

[2] W. H. Press, *Numerical recipes in C the art of scientific computing*, Second ed. Cambridge etc.: Cambridge University Press, 1999.

[3] S. V. Kartalopoulos, *DWDM networks, devices, and technology*. Piscataway, NJ: IEEE Press, 2003.

[4] A. Leon-Garcia and I. Widjaja, *Communication networks fundamental concepts and key architectures*. Boston, Mass.: McGraw-Hill, 2000.

[5] F. Frhr. v. Loeffelholz, "Pionier der Informationstheorie Claude Elwood Shannon," *c't - Magazin für Computertechnik,* vol. 6/2001, 2001.

[6] P. J. Winzer, "Modulation and Multiplexing in Optical Communications," in *Conference on Lasers and Electro-Optics/International Quantum Electronics Conference*, Baltimore, Maryland, 2009, p. CTuL3.

[7] W. Freude, R. Schmogrow, D. Hillerkuss, J. Meyer, M. Dreschmann, B. Nebendahl*, et al.*, "Reconfigurable optical transmitters and receivers," 2012, pp. 82840A-82840A-8.

[8] *Twisted-Pair-Kabel*. Available: <http://de.wikipedia.org/wiki/Twisted-Pair-Kabel>

[9] *Kabel - nicht nur für den Computerbau wichtig*. Available: <http://www.hardware-bastelkiste.de/index.html?cable.html#TP%E2%80%9C>

[10] A. Leon-Garcia and I. Widjaja, "Twisted Pair," in *Communication networks fundamental concepts and key architectures*, ed Boston, Mass.: McGraw-Hill, 2000, p. 148.

[11] T. Kremp and W. Freude, "DWDM transmission optimization in nonlinear optical fibres with a fast split-step wavelet collocation method," in *7th International Conference on Optoelectronics, Fiber Optics & Photonics (Photonics)*, Kochi, India, 2004.

[12] R.-J. Essiambre, G. J. Foschini, P. J. Winzer, and G. Kramer, "Capacity limits of fiber-optic communication systems," in *Proc. Opt. Fiber Commun. Conf.*, San Diego, CA, 2009.

[13] *Video broadcasting technology*. Available: <http://www.epanorama.net/links/videobroadcasting.html>

[14] *High-definition television*. Available: <http://en.wikipedia.org/wiki/High-definition_television>

[15] P. Qu and C. Polley. (2005). *The New Standard-Bearer: China is now trying to set the rules for many developing technologies*. Available: <http://spectrum.ieee.org/computing/hardware/the-new-standardbearer>

[16] D. Santa-Cruz and T. Ebrahimi, "A study of JPEG 2000 still image coding versus other standards," *Proc. of the X European Signal Processing Conference,* vol. 2, pp. 673-676, 2000.

1. List of Symbols

Text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text.

Text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text text.